**TOWER CLOCK**

**TIME CONTROLLER**

**NORMAL TIME**

3.875” (3 7/8”)

**FAST**

**FORWARDS**

**FAST BACKWARDS**

ROLAND HOROLOGY

2.75”

NOTES:

Stainless Steel

Outer edge is line to “cut on”.

Inner, thicker line should remain on faceplate as an “outline” inset from the edge

4 holes to be drilled in each corner: 1/8” dia.

Center hole for potentiometer drilled: ¼” dia

Qty 10 faceplates needed

Final design may change a little (font, text, layout, etc), nothing that should affect quote

Will provide final design via PDF without dimensions and notes